Questions & Answers for QSP 26-02 Floor Coverings

1. Glue-Down Plank (LVP/LVT): The specification allows 2.0–3.0 mm thickness and wear layers ranging from 6 mil to 20+ mil. This represents a significant difference in product grade and cost. Can GDPM provide a minimum required thickness and wear layer, or a basis-of-bid product, so all bidders are pricing comparable material? Or would you perfer we bid all 3 -  6mil, 12, mil, and 20 mil as these are the standard ratings?
Answer: Cost pricing sheet has been amended and an addendum has been issued regarding the plank thickness, wear layer, and pricing.

1. Subfloor Preparation: Please clarify how subfloor preparation will be authorized and billed. Patching, skim coating, are much less labor and material than leveling.  Do you want us to bid them out as two separate types of labor and materials?
Answer: Cost pricing sheet has been amended and an addendum has been issued regarding subfloor prep and pricing.

